Minutes of Functional Design Phase

15:12:04 11:50
Present:

Ebenezer, 
Marketing Expert

Tarik,

Industrial Designer

Dave,

User Interface Designer

Adam,

Project Manager

Agenda :

1. Overview of previous minutes

2. Addition of new requirements

3. Presentations from the various sections

4. Analysis and design decisions

1. Previous minutes stated. Quick reminder of previous decisions made

2. Management have put forward 3 new requirements on this design. They are

1. Teletext has become outdated, due to the popularity of the Internet.

2. The remote control should only be used for the television, otherwise the project becomes more complex, which endangers the time-to-market. 

3. Our corporate image should stay recognizable in our products. Our corporate color and slogan must be implemented in the new design.

3. Presentations

Marketing Expert : People lose remote controls, Potential for voice activated. Certain functions are very common compared to others

User Interface designer : Comparison of two methodologies. Many keys or limited functionality. Proposal of LCD and joystick for navigation.

Industrial designer : Overview of current designs and areas where decisions are required.
4. Analysis and design decisions

The option of voice activation was interesting but placed as impractical due to performance and cost. The idea of a LCD and joystick was instead chosen based on users previous use of mobile phones. This small number of buttons should allow for a wide range of designs to allow the product to stand out. The concept of losing the RC was pursued and it was decided to include a design that allows audio and visual localization. This would be activated by a device placed on the side of the TV or if a deal with a manufacturing company is met then inside the TV .

Remote Control requirements are as follows

1. Monochrome LCD large enough to comfortably show enough information for navigation.

2. Dual-purpose joystick for either navigating LCD display or up-down function for volume and left-right for channel switching.

3. Power button in addition to 2 other buttons. One to start LCD navigation and another to confirm selection.

4. Small (possibly battery operated) transmitter for locating the RC if lost. Transmitter to be secured somewhere to be chosen by user

5. Speaker and bright LED to be used to allow location when transmitter is used.

6. Design to be in keeping with ergonomics but still unique and including company logo

